- Fast PC DAQ Boards 8 to 16 bit, up to 500 MS/s, 4 GB Wide range for PCI, PCIX, PXI, cPCI www.spectrum-instrumentation.com

- Extend Your Battery Life with PIC MCUs from Microchip 20nA Sleep Current www.microchip.com/xlp

- x86 Embedded uControllers ADC/DAC, motion, LCD, I/O, Ethernet Low-Cost, Flexible, C/C++ Program www.tern.com

- Zelix KlassMaster The Heavy Duty Java Obfuscator Smaller Bytecode & Extra protection www.zelix.com

- Bit Mask Calculator For mobile phones and mp3 players Get Hex AND, OR Masks from Binary www.criticalvelocity.com/software